This download contains the BIOS, BMC (Baseboard Management Controller), and FRUSDR updates for the Intel® Server Board SCB2 ATA/SCSI serverboard.

Extraction Instructions:
1. Prepare 3 blank bootable formatted floppy disks.
2. Label them as BIOS2.0; BMCv0.56; & FRUSDR5.0.P.
3. Download the file (BIOS2_BMC56_FRUSDR50P.EXE) into a temporary directory (c:\temp).
4. Extract the file, it will produce three files: (BIOS2.EXE, BMC56.EXE, and FRUSDR_50P.EXE).
5. Extract the BIOS2.EXE into a temporary directory (e.g. c:\temp). It will produce 4 files.
6. Run BIOS.EXE A: on a command prompt to extract the files on the floppy disk (created in step 1 labeled BIOS2.0).
7. Extract the BMC56.EXE into the floppy disk (created in step 1 labeled BMCv0.56).
8. Extract the FRUSDR_50P.EXE into a temporary directory (e.g. c:\temp). It will produce 2 files.
9. Extract the file named FCBV50BP.EXE to the floppy disk (created in step 1 labeled FRUSDR5.0.P).
10. When doing the update, please update the BMC first and then the FRUSDR next, and the BIOS last.

Important Notes:

PLEASE READ THE RELEASE NOTES IN EACH FILE BEFORE DOING THE UPDATES.

BMC Update - BMC firmware version 0.56 is ONLY compatible for use with SCB2 BIOS Production 2.0 build 39 or later and FRUSDR 5.0.P or later. The SCB2 BMC firmware version 0.56 is not backward compatible with any previous releases of BIOS or FRUSDR.

FRUSDR - This package is for use with SCB2 BMC 56 or later only, and SCB2 BIOS Production 2 build 39 and later only. It is not compatible for use with previously released versions of SCB2 BMC firmware and BIOS.

BIOS - This version of SCB2 BIOS is only compatible for use with SCB2 BMC firmware rev 0.56 or later and FRUSDR 5.0.P or later. It is NOT backward compatible with previous version of BMC firmware and FRUSDR packages. This version of SCB2 BIOS is not compatible for use with ISC 3.5.1. This BIOS will only support ISC version 3.5.2.

The BIOS bootblock MUST be updated before updating the BIOS operational code. The BIOS Boot Block and operational code can be updated by typing the following commands at the DOS prompt:

(Note: No baseboard jumper changes are needed to perform this operation)

A> IFLASH.EXE /P P10-0039.BBO
A> 1.BAT