Detailed Description

This file contains the following BIOS/Firmware revisions:

BMC 0.63
FRU/SDR 5.0.P
BIOS Production Release 2.12 Build 77
HSC 0.07 for the Intel® Server Chassis SR1200 SCSI SKU only.
HSC 0.05 for the Intel® Server Chassis SR2200

Instructions:

1. Prepare a blank formatted floppy disk.
2. Extract the contents of SUP executable file to the formatted floppy disk created in step 1.
3. Boot the server from the "SERVER BOARD RESOURCE CD" that shipped with the Intel® Server.
4. After booting from the CD, select "QUIT TO DOS" from the menu.
5. Place the System Update Package disk in the A: drive and type the command A:\SETUP.BAT then press ENTER.